nvme-micron-clear-pcie-errors(1)
===============================

NAME
----
nvme-micron-clear-pcie-errors - Clears correctable PCIe correctable errors of given Micron device

SYNOPSIS
--------
[verse]
'nvme micron clear-pcie-correctable-errors' <device>

DESCRIPTION
-----------
This command clears corretable pcie errors for the specified Micron device.

The <device> parameter is mandatory and may be either the NVMe
character device (ex: /dev/nvme0), or a namespace block device (ex:
/dev/nvme0n1). 

This will only work on Micron devices devices of model numbers 54XX. Support for new
devices may be added subsequently.

OPTIONS
-------
None

EXAMPLES
--------
* Retrieve NAND statistics information
+
------------
# nvme micron clear-pcie-correctable-errors /dev/nvme0

------------

NVME
----
Part of the nvme-user suite
