nvme-dera-stat(1)
=================

NAME
----
nvme-dera-stat - Send NVMe Dera Device status and Additional SMART log page request, returns result and log

SYNOPSIS
--------
[verse]
'nvme dera stat' <device> 

DESCRIPTION
-----------
Retrieves the NVMe Dera Device status and Additional SMART log page from the device and
provides the returned structure.

The <device> parameter is mandatory and may be either the NVMe character
device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the returned status and smart log structure are printed in a readable format.

OPTIONS
-------
none


EXAMPLES
--------
* Print the Dera Device status and Additional SMART log page in a human readable format:
+
------------
# nvme dera stat /dev/nvme0
------------

NVME
----
Part of the nvme-user suite
