nvme-endurance-log(1)
=====================

NAME
----
nvme-endurance-log - Send NVMe Endurance log page request, returns result and log

SYNOPSIS
--------
[verse]
'nvme endurance-log' <device> [--group-id=<group> | -g <group>]
			[--output-format=<fmt> | -o <fmt>]

DESCRIPTION
-----------
Retrieves the NVMe Endurance log page from an NVMe device and provides the returned structure.

The <device> parameter is mandatory and may be either the NVMe character
device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the returned endurance log structure may be returned in one of
several ways depending on the option flags; the structure may parsed by
the program and printed in a readable format, the raw buffer may be
printed to stdout for another program to parse, or reported in json format.

OPTIONS
-------
-g <group>::
--group-id=<group>::
	The endurance group identifier.

-o <format>::
--output-format=<format>::
              Set the reporting format to 'normal', 'json', or
              'binary'. Only one output format can be used at a time.

EXAMPLES
--------
* Print the Endurance log page in a human readable format:
+
------------
# nvme endurance-log /dev/nvme0
------------
+

* Print the raw Endurance log to a file:
+
------------
# nvme endurance-log /dev/nvme0 --output=binary > endurance_log.raw
------------
+
It is probably a bad idea to not redirect stdout when using this mode.

NVME
----
Part of the nvme-user suite
